{"text_format":"5","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"props":{"creator":"Bohlmann","last_modified_by":"Bohlmann","company":"Uranus"},"read":"whole","wrapped":"gz","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":118,"n_cols":13,"rows_kept":118,"flags":["formulas_cached_only"]}
["Telefonkarte",{"$nulls":7},"Preis"]
["Halbleiter",{"$nulls":3},"Pins","Bohrungen",null,null,"Segor, Berlin","Reichelt","Conrad"]
[1,"DS80C320","DIL40","IC1",40,40,null,null,{"v":24,"d":"24.00 DM"},{"$nulls":3},{"v":24,"d":"24.00 DM"}]
[1,"74ACT573","DIL20","IC2",20,20,null,null,{"v":1.5,"d":"1.50 DM"},{"$nulls":3},{"v":1.5,"d":"1.50 DM"}]
[1,"27C512-100","DIL28 prog.","IC3",28,28,null,null,{"v":4.8,"d":"4.80 DM"},{"$nulls":3},{"v":4.8,"d":"4.80 DM"}]
[1,"62C256-70","DIL28","IC4",28,28,null,null,{"v":5.5,"d":"5.50 DM"},{"$nulls":3},{"v":5.5,"d":"5.50 DM"}]
[1,"M48T08-100","DIL28+Batt.","IC5",28,28,null,null,{"v":42,"d":"42.00 DM"},{"$nulls":3},{"v":42,"d":"42.00 DM"}]
[1,"AM79C30A","PLCC44","IC6",44,44,null,null,{"v":49,"d":"49.00 DM"},{"$nulls":3},{"v":49,"d":"49.00 DM"}]
[1,"74C922/3","DIL18/20","IC7",20,20,null,null,{"v":16.6,"d":"16.60 DM"},{"$nulls":3},{"v":16.6,"d":"16.60 DM"}]
[1,"74ACT139","DIL16","IC8",16,16,null,null,{"v":0.9,"d":"0.90 DM"},{"$nulls":3},{"v":0.9,"d":"0.90 DM"}]
[2,"74ACT00","DIL14","IC9, IC10",14,28,null,null,{"v":0.8,"d":"0.80 DM"},{"$nulls":3},{"v":1.6,"d":"1.60 DM"}]
[1,"TL074","DIL14","IC11",14,14,null,null,{"v":1.6,"d":"1.60 DM"},{"$nulls":3},{"v":1.6,"d":"1.60 DM"}]
[1,"TDA7050","DIL8","IC12",8,8,null,null,{"v":2.8,"d":"2.80 DM"},{"$nulls":3},{"v":2.8,"d":"2.80 DM"}]
[1,"LM2575HVN","DIL16","IC13",16,16,null,null,{"v":10.6,"d":"10.60 DM"},{"$nulls":3},{"v":10.6,"d":"10.60 DM"}]
[3,"MBR160","RM10","D10, D11, D12",2,6,null,null,{"v":0.6,"d":"0.60 DM"},{"$nulls":3},{"v":1.7999999999999998,"d":"1.80 DM"}]
[1,"1N4148","RM7,5","D20",2,2,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.1,"d":"0.10 DM"}]
[8,"1N4001","RM10","D31-D38",2,16,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.8,"d":"0.80 DM"}]
[1,"Q=11,052MHz","RM5","Q1",2,2,null,null,{"v":1.8,"d":"1.80 DM"},{"$nulls":3},{"v":1.8,"d":"1.80 DM"}]
[1,"Q=12,288MHz","RM5","Q2",2,2,null,null,{"v":1.8,"d":"1.80 DM"},{"$nulls":3},{"v":1.8,"d":"1.80 DM"}]
[1,"Q=3,5795MHz","RM5","Q3",2,2,null,null,{"v":1.8,"d":"1.80 DM"},{"$nulls":3},{"v":1.8,"d":"1.80 DM"}]
["Widerstände:"]
[1,"10","RM7,5","R60",2,2,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.1,"d":"0.10 DM"}]
[4,"24","RM7,5","R35-R38",2,8,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.4,"d":"0.40 DM"}]
[1,"100","RM7,5","R63",2,2,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.1,"d":"0.10 DM"}]
[6,"1,0k","RM7,5","R44-R47, R50, R51",2,12,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.6000000000000001,"d":"0.60 DM"}]
[1,"2,2k","RM7,5","R62",2,2,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.1,"d":"0.10 DM"}]
[4,"2,7k","RM7,5","R31-R34",2,8,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.4,"d":"0.40 DM"}]
[16,"10k","RM7,5","R20, R30, R33, R39, R40-R43, R52-R57, R70",2,32,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":1.6,"d":"1.60 DM"}]
[2,"100k","RM7,5","R58, R59",2,4,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.2,"d":"0.20 DM"}]
[1,"1,0M","RM7,5","R61",2,2,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.1,"d":"0.10 DM"}]
[1,"4 x 4,7k","SIL5","RN1",5,5,null,null,{"v":0.3,"d":"0.30 DM"},{"$nulls":3},{"v":0.3,"d":"0.30 DM"}]
[1,"Poti=10k","P-10 liegend","P5",3,3,null,null,{"v":0.6,"d":"0.60 DM"},{"$nulls":3},{"v":0.6,"d":"0.60 DM"}]
[2,"Poti=22k","P-10 liegend","P1, P2",3,6,null,null,{"v":0.6,"d":"0.60 DM"},{"$nulls":3},{"v":1.2,"d":"1.20 DM"}]
[2,"Poti=470k","P-10 liegend","P3, P4",3,6,null,null,{"v":0.6,"d":"0.60 DM"},{"$nulls":3},{"v":1.2,"d":"1.20 DM"}]
["Kapazitäten:"]
[6,"15pF","RM2,5","C21, C22, C31, C32, C61, C62",2,12,{"$nulls":6},0]
[4,"100pF","RM2,5","C52, C53, C56, C57",2,8,{"$nulls":6},0]
[1,"1,0nF","RM2,5","C45",2,2,{"$nulls":6},0]
[1,"2,2nF","RM2,5","C30",2,2,{"$nulls":6},0]
[20,"100nF","RM2,5","C33, C43-C45, C52, C53, C58, C59, C101-C112",2,40,{"$nulls":3},{"v":0.14,"d":"0.14 DM"},null,null,{"v":2.8000000000000003,"d":"2.80 DM"}]
[1,"220nF","RM5","C72",2,2,{"$nulls":6},0]
[2,"1,0F","RM2,5","C54, C55",2,4,{"$nulls":6},0]
[7,"2,2F","RM2,5 tant.","C20, C71",2,14,{"$nulls":6},0]
[2,"47F / 6V","RM2,5","C41, C42",2,4,{"$nulls":6},0]
[1,"100F / 6V","RM2,5","C40",2,2,{"$nulls":6},0]
[1,"100F / 60V","RM5","C10",2,2,{"$nulls":6},0]
[2,"470F / 6V","RM5","C11",2,4,{"$nulls":6},0]
["Induktivitäten:"]
[1,"ZKB 5051/X005","ISDN-ÜTr.","TR1",2,2,null,null,{"v":26,"d":"26.00 DM"},{"$nulls":3},{"v":26,"d":"26.00 DM"}]
[1,"1000H / 2A","RM10","L10",4,4,{"$nulls":6},0]
["Sockel / Steckverbinder:"]
[1,"44 pol.","PLCC","IC6",null,0,null,null,{"v":1.8,"d":"1.80 DM"},{"$nulls":3},{"v":1.8,"d":"1.80 DM"}]
[1,"40 pol.","DIL","IC1",null,0,null,null,{"v":2,"d":"2.00 DM"},{"$nulls":3},{"v":2,"d":"2.00 DM"}]
[3,"28 pol.","DIL","IC3, IC4, IC5",null,0,null,null,{"v":1.4,"d":"1.40 DM"},{"$nulls":3},{"v":4.199999999999999,"d":"4.20 DM"}]
[2,"20 pol.","DIL","IC2, IC7",null,0,{"$nulls":6},0]
[2,"16 pol.","DIL","IC8, IC13",null,0,{"$nulls":6},0]
[3,"14 pol.","DIL","IC9, IC10, IC11",null,0,{"$nulls":6},0]
[1,"8 pol.","DIL","IC12",null,0,{"$nulls":6},0]
[1,"2 x 7 Stecker","RM2,54","X1",14,14,{"$nulls":6},0]
[1,"1 x 9 Stecker","RM2,54","X2",9,9,{"$nulls":6},0]
[1,"1 x 7 Stecker","RM2,54","X12",7,7,{"$nulls":6},0]
[2,"1 x 6 Stecker","RM2,54","X3, X11",6,12,{"$nulls":6},0]
[1,"1 x 5 Jumper","RM2,54","JP1",5,5,{"$nulls":6},0]
[3,"1 x 4 Stecker","RM2,54","X4, X5, X6",4,12,{"$nulls":6},0]
[1,"1 x 3 Stecker","RM2,54","JP2",3,3,{"$nulls":6},0]
[1,"1 x 2 Stecker","RM2,54","X7",2,2,{"$nulls":6},0]
[{"$nulls":5},578,34.68,{"$nulls":5},0]
["DSP-Karte"]
["Halbleiter:"]
[2,"TMS320C26B","PLCC44","IC1, IC2",68,136,null,null,{"v":59,"d":"59.00 DM"},{"$nulls":3},{"v":118,"d":"118.00 DM"}]
[1,"Osc=40MHz","DIL14 / 4","IC3",4,4,null,null,{"v":6.8,"d":"6.80 DM"},{"$nulls":3},{"v":6.8,"d":"6.80 DM"}]
[1,"74HCT157","DIL16","IC4",16,16,null,null,{"v":0.8,"d":"0.80 DM"},{"$nulls":3},{"v":0.8,"d":"0.80 DM"}]
[1,"74HCT86","DIL14","IC5",16,16,null,null,{"v":0.6,"d":"0.60 DM"},{"$nulls":3},{"v":0.6,"d":"0.60 DM"}]
["Widerstände:"]
[2,"100","RM7,5","R1, R2",2,4,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.2,"d":"0.20 DM"}]
[2,"10k","RM7,5","R3, R4",2,4,null,null,{"v":0.1,"d":"0.10 DM"},{"$nulls":3},{"v":0.2,"d":"0.20 DM"}]
[2,"6 x 10k","SIL7","RN1, RN2",7,14,null,null,{"v":0.4,"d":"0.40 DM"},{"$nulls":3},{"v":0.8,"d":"0.80 DM"}]
["Kapazitäten:"]
[5,"100nF","RM2,5","C1-C5",2,10,{"$nulls":3},{"v":0.14,"d":"0.14 DM"},null,null,{"v":0.7000000000000001,"d":"0.70 DM"}]
[null,"Sockel / Steckverbinder:",{"$nulls":10},0]
[2,"68 pol","PLCC","IC1, IC2",{"$nulls":4},{"v":2.1,"d":"2.10 DM"},{"$nulls":3},{"v":4.2,"d":"4.20 DM"}]
[1,"16 pol","DIL","IC4",{"$nulls":8},0]
[1,"14 pol","DIL","IC5",{"$nulls":8},0]
[1,"4 pol","DIL14 / 4","IC3",{"$nulls":8},0]
[2,"2 pol","RM2,54","JP1, JP2",2,4,{"$nulls":6},0]
[1,"1 x 7 Buchse","RM2,54","X2",7,7,{"$nulls":6},0]
[1,"1 x 6 Buchse","RM2,54","X1",6,6,{"$nulls":6},0]
[{"$nulls":5},221,13.26]
[1,"LC-Display 2x40 mit 14-poliger Verbindungsleitung",{"$nulls":7},{"v":69,"d":"69.00 DM"},null,null,{"v":69,"d":"69.00 DM"}]
[1,"Matrix-Tastatur 4x4 / 5x4 mit 8/9-poliger Verbindungsleitung",{"$nulls":10},0]
[1,"Chipkarten-Schacht mit 6-poliger Verbindungsleitung",{"$nulls":6},{"v":18.9,"d":"18.90 DM"},{"$nulls":3},{"v":18.9,"d":"18.90 DM"}]
[1,"zwei Lautsprecher mit einer 4-poligen Verbindungsleitung",{"$nulls":6},{"v":4,"d":"4.00 DM"},{"$nulls":3},{"v":4,"d":"4.00 DM"}]
[1,"zwei Mikrofone mit einer 4-poliger Verbindungsleitung",{"$nulls":6},{"v":2.5,"d":"2.50 DM"},{"$nulls":3},{"v":2.5,"d":"2.50 DM"}]
[1,"Taster/Schalter mit 2-poliger Verbindungsleitung",{"$nulls":10},0]
[{"$nulls":9},"Bauteile",null,null,{"v":439.40000000000003,"d":"439.40 DM"}]
[{"$nulls":9},"Platinen",null,null,{"v":232.09279999999998,"d":"232.09 DM"}]
[{"$nulls":9},"Preis ohne Gehäuse",null,null,{"v":671.4928,"d":"671.49 DM"}]
[null,"Platine Telefon"]
[null,160," Quadratzentimeter Platinenfläche  x DM 0,10 ",null,{"v":16,"d":"16.00 DM"}]
[null,578," Bohrungen x DM 0,06 ",null,{"v":34.68,"d":"34.68 DM"}]
[null,null,"Zuschlag 50% für doppelseitige Platine",null,{"v":25.37,"d":"25.37 DM"}]
[null,6," Werkzeuge x DM 2,-- ",null,{"v":12,"d":"12.00 DM"}]
[null,null,"Platinenpreis",null,{"v":88.05,"d":"88.05 DM"}]
[null,null,"Outline-Erstellung (einmalig)",null,{"v":30,"d":"30.00 DM"}]
[null,null,"Gesamtpreis",null,{"v":118.05,"d":"118.05 DM"}]
[null,null,"16% MWST",null,{"v":18.888,"d":"18.89 DM"}]
[null,null,"Endsumme",null,{"v":136.938,"d":"136.94 DM"}]
[]
[null,"Platine DSP"]
[null,54," Quadratzentimeter Platinenfläche  x DM 0,10 ",null,{"v":5.4,"d":"5.40 DM"}]
[null,221," Bohrungen x DM 0,06 ",null,{"v":13.26,"d":"13.26 DM"}]
[null,null,"Zuschlag 50% für doppelseitige Platine",null,{"v":25.37,"d":"25.37 DM"}]
[null,null," Werkzeuge x DM 2,-- ",null,{"v":8,"d":"8.00 DM"}]
[null,null,"Platinenpreis",null,{"v":52.03,"d":"52.03 DM"}]
[null,null,"Outline-Erstellung (einmalig)",null,{"v":30,"d":"30.00 DM"}]
[null,null,"Gesamtpreis",null,{"v":82.03,"d":"82.03 DM"}]
[null,null,"16% MWST",null,{"v":13.1248,"d":"13.12 DM"}]
[null,null,"Endsumme",null,{"v":95.1548,"d":"95.15 DM"}]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}